Switch to Russian

## LtSpice/SwCADIII

Linear Technologies makes very nice Spice simulator which is a) free; b) reliable; c) updated on weekly basis (so if you experience issues they'll be fixed rapidly) and d) has one of the -- if not the -- fastest, precise and numerically stable solvers (it it recommended to go to Tools->Contol Panel->Spice and choose Solver->Alternate).

One of the major problems with SwCAD is lack of standard elements (though the library of LT chips is quite impressive); you can download my library of elements. Most of them are obtained from respective manufacturers' web cites, some were borrowed from Yahoo LTSpice group, so were provided by private parties. I admit that in the latter case I often slightly modified the schematics so that the element's symbol and other files do not need to be copied into the same directory with the schematics (the path to respective spice library file is embeeded into the symbol), the user does not need to enter model name (it is embedded into the symbol), and, in couple of cases, corrected the problem of using node 0 (global ground) inside subcircuit. Except for these rare and minor changes, I tried by best to retain original files with all the copyrights and references to the part manufacturer and/or circuit owner.

## Additional elements for SwCAD

- Attention: installation will overwrite \SwCADIII\lib\cmp\standard.{bjt,dio,mos,jft} files, so if you added your own bipolar transistor, diode, MOSFET, or JFET models, you'd better back them up and merge with new set later (if you do not understand what this all is about, do not worry then -- you will not be affected).
- Make sure that SwCAD is installed in disk root directory (e.g. C:\SwCADIII, not "C:\Program Files\SwCADIII" or whatever).
- Download library of extra elements for SwCAD.
- Unpack "extra.rar" using RAR archiver and get "extra1.rar".
- Copy "extra1.rar" to the same disk where SwCAD is installed.
- Unpack "extra1.rar" onto the same disk where SwCAD is installed.
- Done.

Switch to English

## LtSpice/SwCADIII

Linear Technologies делает чудный SPICE симулятор под кодовым названием LtSpice aka SwCAD. Чудный потому, что а) бесплатный; бе) надежный; це) ошибки чинятся быстро, обновления -- каждую неделю; де) самый быстрый, точный и устойчивый (сильно рекомендуется пойти в Tools->Contol Panel->Spice и выбрать Solver->Alternate).

Одной из главных проблем с SwCAD является наличие отсутсвия богатой библитеки элементов. Сей пробел был восполнен с помощью производителей микросхем, участников форумов Yahoo LTSpice group и ряда частных лиц, указанных в соответствующих моделях и символах.

## Установка библиотеки дополнительных элементов к SwCAD

- Внимание! Установка перепишет содержимое файлов \SwCADIII\lib\cmp\standard.{bjt,dio,mos,jft}, посему, если Вы добавляли свои модели биполярных транзисторов, диодов, MOSFET-ов, или JFET-ов, Вам лучше сохранить старые версии вышеперечисленных файлов и, после инсталляции, добавить Ваши элементы заново (а если Вы не понимаете, о чем идет речь, тогда и волноваться не о чем, т.к. это к Вам не относится).
- Убедитесь, что SwCAD установлен в корневой директории на диске (н-р, C:\SwCADIII, а не "C:\Program Files\SwCADIII").
- Скачайте библитеку дополинтельных элементов.
- Воспользовавшись архиватором RAR, распакуйте "extra.rar" и получите "extra1.rar".
- Скопируйте "extra1.rar" на тот же диск, где установлен SwCAD.
- Распакуйте "extra1.rar" на тот же диск, где установлен SwCAD.
- Готово.